
RICK HANSEN

AUDIO VISUAL REQUIREMENTS

The Event/Organizers should consider the following:
(event a/v details or modifications are to be confirmed at least 2 weeks before the event)

PA SYSTEM:  ( size must be sufficient to meet the needs of the event)
need to 1 channel for our main headset, 1 channel for our backup wireless handheld, 1 or 2 channels for the audio feeds from our mini DVCam video player.  XLR connector, ¼ phone or RCA connectors are required on the mixer/amp.
LIGHTING SYSTEM:  (stage wash, with fresnels or low spot at larger venues) including access to the controls or via a light technician.  The objective is to get reasonably focused lighting on Rick that does not interfere with the presentation screen.
PROJECTOR DATA/VIDEO & SCREEN (800x600 resolution):  either front or rear projection depending on the event. Screens should be at least 8 ft. or larger. If the projection is to be done on TV Screens then a quality scan rate converter capable of 800x600 resolution is required. It must also support multi-sync frequencies for compatibility. Access to the remote control or the operator is a priority as the presentation changes from Data to Video throughout the show.
Need the cabling to feed our mini video signal to the projector (composite, svideo or IIIE 1394) 

COMPUTER MONITOR:  including a vga cable running up to 50ft. The cable can be a series of cables connected to each other. Quality is not important as the issue of getting the signal to cover the distance from the laptop at the A/V table to the stage monitor. The monitor is placed strategically on stage as a cueing device and connects to the laptop #2 which is located at the A/V table.  This runs separately from the main presentation.
BACKUP HEADSET MICROPHONE:  Lavalier is fine.
EXTENSION CORDS AND ELECTICAL OUTLETS:  with 3 – 4 circuits, if available.  
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The Rick Hansen Institute provides the following:

Microphone System:
Shure UHF wireless microphone system includes: 
1- a countryman wireless headset (main)
1- handheld wireless mic (backup)

Primary Presentation Computer:
Sony Vaio  PIII 500/ using Astound (similar to PowerPoint)
Output resolution 800x600 24 bit colour
This laptop sends a feed to an external Data/Video projector that can operate at 800x600
Secondary Presentation Computer:
Acer P2300/using Astound (similar to PowerPoint)

Output resolution 800x600 24 bit colour

This laptop sends a feed to an external VGA 14" or smaller Computer Monitor.  The purpose of this laptop is to act as an onstage visual cue and runs a slide a head of the main presentation. The unit also acts as a standby in case of failure in primary unit.  This unit has a slightly different version of the main presentation. The event should supply the 14” in or larger VGA monitor and cable (cable length runs from the monitor on stage to the main A/V table where the laptop is situated.)
Projector: Sanyo 700 lumen desktop projector. 800 x 600 resolution.  Can be used for small rooms, or in large rooms where stage lighting is available.  Projector may not be suitable for all presentations.

Sony DSRV10 DVCam player:  We provide this unit along with all our video clips
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